Stripboard Layout Planning Sheet

Project:
Designed by:
Version:
Date:
Notes:

Actual size stripboard. Hole spacing 0.1” (2.54mm)
Tracks run this way

Tips:
Mark out the Vs and 0V power lines first, then place the ICs.
Remember to cut the track between the pins of an IC. Mark the cuts on the diagram with an X.
Try to make resistors and axial capacitors lay flat on the stripboard. Resistors usually require a gap of 4 holes, capacitors a gap of 8 holes.
Use the actual size grid on the left to check component spacing.
Number the pins of the ICs as shown.

1

2

3

4

5

6

7

8

9

10

11

12

13

14

15

16

17

18

19

20

21

22

23

24

25

26

27

287

29

30

31

32

33

34

35

36

37

38

39

40

41

42

43

44

1

2

3

4

5

6

7

8

9

10

11

12

13

14

15

16

17

18

19

20

21

22

23

24

25

26

27

287

29

30

31

32

33

34

35

36

37

38

39

40

41

42

43

44

1

2

3

4

5

6

7

8

9

10

11

12

13

14

15

16

17

18

19

20

21

22

1

2

3

4

5

6

7

8

9

10

11

12

13

14

15

16

17

18

19

20

2l1

22

1
2
3
4

8
7
6
5

Version 3 : 3/02 © 2002 Electronics in Meccano www.eleinmec.com